#
# fhem.pl configfile
# 
# Define a lamp (which is plugged in via an FS20ST).
# To program the FS20ST, start the server, plug the FS20ST while pressing its
# button (it starts blinking), and then execute   fhem.pl 7072 "set lamp on" 
#

# Common part
attr global logfile /tmp/fhem-%Y-%m.log
attr global statefile /tmp/fhem.save   # where to save the state of the devices
attr global verbose 3                  # "normal" verbosity (min 1, max 5)
attr global port 7072                  # our TCP/IP port (localhost only)
attr global modpath .                  # where our FHEM directory is

define FHZ FHZ /dev/tts/USB0 # the serial port of an FHZ 1000 PC

define lamp FS20 8765 01    # type FS20, transmitter code 8765, button 2
