#
# pgm2 / autocreate configfile. Take a look at the other examples for more.
#
attr global logfile /tmp/fhem-%Y-%m.log
attr global modpath .                  # where our FHEM directory is
attr global port 7072                  # our TCP/IP port (localhost only)
attr global statefile /tmp/fhem.save   # where to save the state of the devices
attr global verbose 3                  # "normal" verbosity (min 1, max 5)

#define CUL CUL /dev/ttyACM0 1234
#define FHZ FHZ /dev/USB0

define WEB FHEMWEB 8083 global

define WEBphone FHEMWEB 8084 global
attr WEBphone smallscreen

define WEBtablet FHEMWEB 8085 global
attr WEBtablet touchpad

# Fake logfile, to access the global log
define Logfile FileLog /tmp/fhem-%Y-%m.log fakelog

define autocreate autocreate
attr autocreate autosave
attr autocreate device_room %TYPE
attr autocreate filelog /tmp/%NAME-%Y.log
attr autocreate weblink
attr autocreate weblink_room Plots
